IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "Option [BaseQuantities:On]"
Description: "Option [GridExport:On]"
Description: "Option [Assemblies:On]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:Off]"
Description: "Option [SurfaceTreatments:On]"
Description: "Option [LocationBy:0]"
Description: "Option [ViewColors:Off]"
Description: "Option [SectionedSpine:Off]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "250LVS Hjørnesæt.ifc"
Time stamp: "2023-08-03T08:43:16"
Author: "IBF\NielsCS"
Organization: "Structural Designer"
Preprocessor: "IFC Database version: Work"
Originating system: "Tekla Structures 2020 Service Pack 9, IFC Export Version: 4.0.0.0 Jun 21 2021"
Application: "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "IBF\NielsCS" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "IBF\NielsCS" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1691044995 (2023-08-03T06:43:15Z)
  Owner history of Person "Undefined" id "IBF\NielsCS" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1691049600 (2023-08-03T08:00:00Z)
  Owner history of Person "Undefined" id "IBF\NielsCS" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1618923600 (2021-04-20T13:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Undefined"
  IFCSITE "Undefined"
    IFCBUILDING "Undefined"
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
        contains 2 elements
          2 x IFCELEMENTASSEMBLY | REINFORCEMENT_UNIT | names: "250LV STD" | parts: 28 IFCELEMENTASSEMBLY, 24 IFCBEAM, 2 IFCWALL | property sets: BaseQuantities, Tekla Assembly

Property sets
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/7" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+1.510" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+1.530" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/4" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+1.477" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+1.564" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/8" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+0.010" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.130" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/4" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+0.000" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.047" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/6" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+0.078" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.099" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/6" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+0.077" (IFCLABEL)
    Assembly/Cast unit position code = "250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.098" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/6" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+0.077" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.098" (IFCLABEL)
    Assembly/Cast unit weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "LE/12(?)" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "-0.000" (IFCLABEL)
    Assembly/Cast unit position code = "250LV-250LV/HV-HH" (IFCLABEL)
    Assembly/Cast unit top elevation = "+2.500" (IFCLABEL)
    Assembly/Cast unit weight = 3345.2 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Cast unit type = "Precast" (IFCLABEL)
    Control number (no value)
  Tekla Assembly: 15 more contents on 15 objects not shown
  BaseQuantities | quantities | on 12 objects (12 IFCELEMENTASSEMBLY)
    Width = 21. [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCELEMENTASSEMBLY)
    Width = 20. [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCELEMENTASSEMBLY)
    Width = 87. [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (4 IFCBEAM, 4 IFCCOLUMN)
    Length = 47. [MILLI METRE]
    NetVolume = 0.000152107666666667 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.0203204341272583 [SQUARE_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCBEAM)
    Length = 100.000000000074 [MILLI METRE]
    NetVolume = 1.00000000000074E-07 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.000402000000000295 [SQUARE_METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    Length = 99.9999999999691 [MILLI METRE]
    NetVolume = 9.99999999999691E-08 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.000401999999999876 [SQUARE_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCBEAM)
    Length = 100.000000000076 [MILLI METRE]
    NetVolume = 1.00000000000076E-07 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.000402000000000306 [SQUARE_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCBEAM)
    Length = 99.9999999999698 [MILLI METRE]
    NetVolume = 9.99999999999698E-08 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.000401999999999879 [SQUARE_METRE]
  BaseQuantities: 17 more contents on 27 objects not shown
  Tekla Common | properties | on 12 objects (12 IFCBEAM)
    Bottom elevation = "+0.038" (IFCLABEL)
    Class = "9" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.138" (IFCLABEL)
  Tekla Common | properties | on 12 objects (12 IFCBEAM)
    Bottom elevation = "+0.087" (IFCLABEL)
    Class = "9" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.088" (IFCLABEL)
  Tekla Common | properties | on 8 objects (8 IFCBEAM)
    Bottom elevation = "+0.077" (IFCLABEL)
    Class = "13" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.098" (IFCLABEL)
  Tekla Common | properties | on 4 objects (4 IFCCOLUMN)
    Bottom elevation = "+0.010" (IFCLABEL)
    Class = "13" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.130" (IFCLABEL)
  Tekla Common | properties | on 4 objects (4 IFCCOLUMN)
    Bottom elevation = "+0.000" (IFCLABEL)
    Class = "6" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.047" (IFCLABEL)
  Tekla Common | properties | on 4 objects (4 IFCBEAM)
    Bottom elevation = "+1.510" (IFCLABEL)
    Class = "13" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+1.530" (IFCLABEL)
  Tekla Common | properties | on 4 objects (4 IFCBEAM)
    Bottom elevation = "+0.078" (IFCLABEL)
    Class = "13" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.099" (IFCLABEL)
  Tekla Common | properties | on 3 objects (3 IFCBEAM)
    Bottom elevation = "+1.477" (IFCLABEL)
    Class = "6" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+1.564" (IFCLABEL)
  Tekla Common: 3 more contents on 3 objects not shown
  Tekla Quantity | properties | on 24 objects (24 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 12 objects (12 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 21. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 21. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 8 objects (4 IFCBEAM, 4 IFCCOLUMN)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 87. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 47. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 87. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 4 objects (4 IFCCOLUMN)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 4 objects (4 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 1 object (1 IFCWALL)
    Area per tons = 6.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2970. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 20.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 3345.2 (IFCMASSMEASURE) [KILO GRAM]
    Width = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 1 object (1 IFCWALL)
    Area per tons = 6.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2970. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 20.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 3350.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/9(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/5(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/9" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/5" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/1(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/2(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/2" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/8(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/5(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/8" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dummy/5" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Concrete_LE-1/12(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Concrete_LE-1/11" (IFCIDENTIFIER)